From 298278d34b44935768c4e63b010f3c89ddf34580 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 15 Mar 2015 11:10:13 +0000
Subject: cl: move out cs02 changelog

start adding one for cs03

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@482 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 cl-cs02.tex | 52 ++++++++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 52 insertions(+)
 create mode 100644 cl-cs02.tex

(limited to 'cl-cs02.tex')

diff --git a/cl-cs02.tex b/cl-cs02.tex
new file mode 100644
index 0000000..61aa6fd
--- /dev/null
+++ b/cl-cs02.tex
@@ -0,0 +1,52 @@
+448 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-120: virtio:
+fix used element size
+
+General ring description lists size for
+used ring elements as 4, it must be 8.
+
+See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
+ } \\
+\hline
+449 & 22 Doc 2014 & Cornelia Huck & {VIRTIO-125: block: fixup section levels
+    The specification for the configuration layout for block devices
+    should be its own subsection as for all other devices and not be
+    hidden beneath "Feature bits".
+    
+    The normative sections for device operation should appear under
+    the device operation section.
+See \ref{sec:Device Types / Block Device / Device configuration
+layout}.
+ } \\
+\hline
+450 & 22 Dec 2014 & Cornelia Huck & {VIRTIO-127: ccw: two-stage
+indicators for legacy devices
+
+    Some legacy devices will support two-stage queue indicators
+and therefore
+    won't reject CCW_CMD_SET_IND_ADAPTER. Note this.
+
+See \ref{sec:Virtio Transport Options / Virtio over channel I/O /
+Device Initialization / Setting Up Indicators / Legacy
+Interfaces: A Note on Setting Up Indicators}.
+ } \\
+\hline
+452 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-115:
+formatting: escape {\textbackslash}ldots in lstlisting
+
+    {\textbackslash}ldots does not work within lstlisting, the result is
+    {\textbackslash}ldots verbatim in the PDF output.
+
+    To fix, make \$ an escape character, and escape the sequence:
+    \${\textbackslash}ldots\$
+
+See \ref{sec:Device Types / SCSI Host Device / Device Operation /
+Device Operation: controlq}.
+} \\
+\hline
+455,457 & 23 Dec 2014 & Michael S. Tsirkin & {acknowledgements: acknowledge dgilbert
+    
+    Acknowledge David Alan Gilbert for reporting VIRTIO-120.
+
+See \ref{chap:Acknowledgements}.
+} \\
+\hline
-- 
cgit v1.2.3

