From 298278d34b44935768c4e63b010f3c89ddf34580 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 15 Mar 2015 11:10:13 +0000
Subject: cl: move out cs02 changelog

start adding one for cs03

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@482 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 cl-os.tex | 58 ++++++++--------------------------------------------------
 1 file changed, 8 insertions(+), 50 deletions(-)

(limited to 'cl-os.tex')

diff --git a/cl-os.tex b/cl-os.tex
index 61aa6fd..9abd1f4 100644
--- a/cl-os.tex
+++ b/cl-os.tex
@@ -1,52 +1,10 @@
-448 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-120: virtio:
-fix used element size
-
-General ring description lists size for
-used ring elements as 4, it must be 8.
-
-See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
- } \\
-\hline
-449 & 22 Doc 2014 & Cornelia Huck & {VIRTIO-125: block: fixup section levels
-    The specification for the configuration layout for block devices
-    should be its own subsection as for all other devices and not be
-    hidden beneath "Feature bits".
-    
-    The normative sections for device operation should appear under
-    the device operation section.
-See \ref{sec:Device Types / Block Device / Device configuration
-layout}.
- } \\
-\hline
-450 & 22 Dec 2014 & Cornelia Huck & {VIRTIO-127: ccw: two-stage
-indicators for legacy devices
-
-    Some legacy devices will support two-stage queue indicators
-and therefore
-    won't reject CCW_CMD_SET_IND_ADAPTER. Note this.
-
-See \ref{sec:Virtio Transport Options / Virtio over channel I/O /
-Device Initialization / Setting Up Indicators / Legacy
-Interfaces: A Note on Setting Up Indicators}.
+478 & 15 Mar 2015 & Cornelia Huck & {VIRTIO-129: legacy:
+clean up virtqueue layout definitions
+
+Generalize "Legacy Interfaces: A Note on Virtqueue Layout" to allow
+for different alignment requirements. Have pci and ccw refer to that
+section for legacy devices. Remove the double definition of virtqueue
+alignment (which referred to legacy, but was not tagged as such) from
+the ccw section.
  } \\
 \hline
-452 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-115:
-formatting: escape {\textbackslash}ldots in lstlisting
-
-    {\textbackslash}ldots does not work within lstlisting, the result is
-    {\textbackslash}ldots verbatim in the PDF output.
-
-    To fix, make \$ an escape character, and escape the sequence:
-    \${\textbackslash}ldots\$
-
-See \ref{sec:Device Types / SCSI Host Device / Device Operation /
-Device Operation: controlq}.
-} \\
-\hline
-455,457 & 23 Dec 2014 & Michael S. Tsirkin & {acknowledgements: acknowledge dgilbert
-    
-    Acknowledge David Alan Gilbert for reporting VIRTIO-120.
-
-See \ref{chap:Acknowledgements}.
-} \\
-\hline
-- 
cgit v1.2.3

