From 37648703597b09fa2db9a3db77504e41608ff3c4 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 25 Mar 2015 17:11:36 +0000
Subject: cl: tweak revisions

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@503 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 cl-os.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'cl-os.tex')

diff --git a/cl-os.tex b/cl-os.tex
index 4f16391..05b6dfa 100644
--- a/cl-os.tex
+++ b/cl-os.tex
@@ -56,7 +56,7 @@ See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues /
 The Virtqueue Used Ring}.
  } \\
 \hline
-486 & 15 Mar 2015 & Rusty Russell & {VIRTIO-130:
+487 & 15 Mar 2015 & Rusty Russell & {VIRTIO-130:
 ISR status: Fix incorrect diagram
 
 ISR status capability diagram has the "Device Configuration
@@ -70,7 +70,7 @@ See \ref{sec:Virtio Transport Options / Virtio Over PCI Bus / PCI
 Device Layout / ISR status capability}.
  } \\
 \hline
-486 & 15 Mar 2015 & Rusty Russell & {VIRTIO-133:
+488 & 15 Mar 2015 & Rusty Russell & {VIRTIO-133:
 Change 4.1.5.1.2.1 to device requirement
 
 4.1.5.1.2.1 is incorrectly labelled as a driver requirement; it's
-- 
cgit v1.2.3

