From 930364b1f7237263fc4ef47157cd10b65b08daf6 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 25 Mar 2015 17:11:02 +0000
Subject: cl: list virtio-130

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@501 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 cl-os.tex | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

(limited to 'cl-os.tex')

diff --git a/cl-os.tex b/cl-os.tex
index 05c1f16..64a83a7 100644
--- a/cl-os.tex
+++ b/cl-os.tex
@@ -56,3 +56,17 @@ See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues /
 The Virtqueue Used Ring}.
  } \\
 \hline
+486 & 15 Mar 2015 & Rusty Russell & {VIRTIO-130:
+ISR status: Fix incorrect diagram
+
+ISR status capability diagram has the "Device Configuration
+Interrupt " as bit 0, and the "Queue Interrupt" as bit 1. This is
+the wrong way around: it disagrees with the legacy
+implementations, as well as the spec elsewhere.
+
+All current guests correctly follow the text, fix
+up the diagram to match.
+See \ref{sec:Virtio Transport Options / Virtio Over PCI Bus / PCI
+Device Layout / ISR status capability}.
+ } \\
+\hline
-- 
cgit v1.2.3

