From 0bc9dbd2b501b8e37410344fb9dc645537142ff2 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 25 Mar 2015 17:07:04 +0000
Subject: Change 4.1.5.1.2.1 to device requirement

4.1.5.1.2.1 is incorrectly labelled as a driver requirement; it's
self-evidently referring to the device.

VIRTIO-133

Signed-off-by: Rusty Russell <rusty@rustcorp.com.au>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@488 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 conformance.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'conformance.tex')

diff --git a/conformance.tex b/conformance.tex
index 59193e9..350d2d0 100644
--- a/conformance.tex
+++ b/conformance.tex
@@ -57,7 +57,6 @@ A PCI driver MUST conform to the following normative statements:
 \item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Common configuration structure layout}
 \item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / ISR status capability}
 \item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / PCI configuration access capability}
-\item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
 \item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / MSI-X Vector Configuration}
 \item \ref{drivernormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Notification of Device Configuration Changes}
 \end{itemize}
@@ -162,6 +161,7 @@ A PCI device MUST conform to the following normative statements:
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / ISR status capability}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Device-specific configuration}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / PCI configuration access capability}
+\item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / MSI-X Vector Configuration}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Virtqueue Interrupts From The Device}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Notification of Device Configuration Changes}
-- 
cgit v1.2.3

