From 619a2785480f3275767b81a02cead33aaba4e801 Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Fri, 9 Mar 2018 23:23:34 +0200
Subject: split-ring: generalize text

Update generic text to talk about available/used buffers, not rings.
Move some split-ring specific text to the correct section.

Update conformance section with link to the new conformance clause.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Approved-by: https://www.oasis-open.org/apps/org/workgroup/virtio/ballot.php?id=3177
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/3
---
 conformance.tex | 1 +
 1 file changed, 1 insertion(+)

(limited to 'conformance.tex')

diff --git a/conformance.tex b/conformance.tex
index 55d17b4..e4efe33 100644
--- a/conformance.tex
+++ b/conformance.tex
@@ -38,6 +38,7 @@ A driver MUST conform to the following normative statements:
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / The Virtqueue Descriptor Table}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / The Virtqueue Descriptor Table / Indirect Descriptors}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Virtqueue Interrupt Suppression}
+\item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / The Virtqueue Available Ring}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / The Virtqueue Used Ring}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Virtqueue Notification Suppression}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Supplying Buffers to The Device / Updating idx}
-- 
cgit v1.2.3

