From 711c7742e232597cdf213b45f7c13eee4e6d6bf8 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Thu, 13 Mar 2014 03:14:50 +0000
Subject: VIRTIO-60: avoid vring and VIRTIO_RING.

These are never introduced, so use simpler names: virtq* for structures
and VIRTIO_ for features.

I added two notes about the old names, for helping people coming from
the old spec.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@327 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 conformance.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'conformance.tex')

diff --git a/conformance.tex b/conformance.tex
index 4896729..942afac 100644
--- a/conformance.tex
+++ b/conformance.tex
@@ -252,7 +252,7 @@ REQUIRED level requirements for the legacy interface
 for the transitional devices and drivers.
 
 The requirements for the legacy interface for transitional implementations
-are located in sections named "Legacy Interface" listed below:
+are located in sections named ``Legacy Interface'' listed below:
 \begin{itemize}
 \item Section \ref{sec:Basic Facilities of a Virtio Device /
 Feature Bits / Legacy Interface: A Note on Feature Bits}
-- 
cgit v1.2.3

