From 967ae5275351ddd3ccaed813e35ef63b28965c6e Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Fri, 9 Mar 2018 23:23:31 +0200
Subject: content: move virtqueue operation description

virtqueue operation description is specific to the virtqueue
format. Move it out to split-ring.tex and update all
references.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
Approved-by: https://www.oasis-open.org/apps/org/workgroup/virtio/ballot.php?id=3177
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/3
---
 conformance.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'conformance.tex')

diff --git a/conformance.tex b/conformance.tex
index f59e360..55d17b4 100644
--- a/conformance.tex
+++ b/conformance.tex
@@ -40,9 +40,9 @@ A driver MUST conform to the following normative statements:
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Virtqueue Interrupt Suppression}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / The Virtqueue Used Ring}
 \item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Virtqueue Notification Suppression}
+\item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Supplying Buffers to The Device / Updating idx}
+\item \ref{drivernormative:Basic Facilities of a Virtio Device / Virtqueues / Supplying Buffers to The Device / Notifying The Device}
 \item \ref{drivernormative:General Initialization And Device Operation / Device Initialization}
-\item \ref{drivernormative:General Initialization And Device Operation / Device Operation / Supplying Buffers to The Device / Updating idx}
-\item \ref{drivernormative:General Initialization And Device Operation / Device Operation / Supplying Buffers to The Device / Notifying The Device}
 \item \ref{drivernormative:General Initialization And Device Operation / Device Cleanup}
 \item \ref{drivernormative:Reserved Feature Bits}
 \end{itemize}
-- 
cgit v1.2.3

