From d4f61005cbd9b954cb89056a57dca7762eb4629b Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Thu, 13 Mar 2014 03:13:33 +0000
Subject: VIRTIO-62: Explicit and specific.

Avoid these words where they are redundant.  This also lead me to
notice that we were not consistent in the use of the term
"device-specific configuration" in the PCI section, so cleaned that up
too.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@323 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 conformance.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'conformance.tex')

diff --git a/conformance.tex b/conformance.tex
index dbbfc7d..4896729 100644
--- a/conformance.tex
+++ b/conformance.tex
@@ -159,7 +159,7 @@ A PCI device MUST conform to the following normative statements:
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Common configuration structure layout}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Notification capability}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / ISR status capability}
-\item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Device specific structure}
+\item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Device-specific configuration}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / PCI configuration access capability}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / MSI-X Vector Configuration}
 \item \ref{devicenormative:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Virtqueue Interrupts From The Device}
-- 
cgit v1.2.3

