From 03391618b6256c9dd1c23dced7fa1c730c1982ae Mon Sep 17 00:00:00 2001
From: "cornelia.huck" <cornelia.huck@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 25 Nov 2013 13:13:17 +0000
Subject: content.tex: Fix virtio-ccw cross reference.

Signed-off-by: Cornelia Huck <cornelia.huck@de.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@123 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index b371651..8a1759a 100644
--- a/content.tex
+++ b/content.tex
@@ -2,7 +2,7 @@
 
 A virtio device is discovered and identified by a bus-specific method
 (see the bus specific sections: \ref{sec:Virtio Transport Options / Virtio Over PCI Bus}~\nameref{sec:Virtio Transport Options / Virtio Over PCI Bus},
-\ref{sec:Virtio Transport Options / Virtio Over MMIO}~\nameref{sec:Virtio Transport Options / Virtio Over MMIO} and \ref{sec:Virtio Transport Options / Virtio Over MMIO}~\nameref{sec:Virtio Transport Options / Virtio Over MMIO}).  Each
+\ref{sec:Virtio Transport Options / Virtio Over MMIO}~\nameref{sec:Virtio Transport Options / Virtio Over MMIO} and \ref{sec:Virtio Transport Options / Virtio Over Channel I/O}~\nameref{sec:Virtio Transport Options / Virtio Over Channel I/O}).  Each
 device consists of the following parts:
 
 o Device Status field
@@ -1705,7 +1705,7 @@ The virtual queue is configured as follows:
 
 Notification mechanisms did not change.
 
-\section{Virtio over channel I/O}\label{sec:Virtio Transport Options / Virtio over channel I/O}
+\section{Virtio Over Channel I/O}\label{sec:Virtio Transport Options / Virtio Over Channel I/O}
 
 S/390 based virtual machines support neither PCI nor MMIO, so a
 different transport is needed there.
-- 
cgit v1.2.3

