From 059b476c6d12aab67174b2c73d4976c7b38990c6 Mon Sep 17 00:00:00 2001
From: Gerd Hoffmann <kraxel@redhat.com>
Date: Thu, 10 Sep 2015 11:18:52 +0200
Subject: Add virtio gpu device specification.

Resuming the effort to get the gpu device specs merged.

Support for 2d mode (3d/virgl mode is not covered by this patch) has
been added to the linux kernel version 4.2 and to qemu version 2.4.

git branch:
  https://www.kraxel.org/cgit/virtio-spec/commit/?h=virtio-gpu

Rendered versions are available here:
  https://www.kraxel.org/virtio/virtio-v1.0-cs03-virtio-gpu.pdf
  https://www.kraxel.org/virtio/virtio-v1.0-cs03-virtio-gpu.html#x1-2800007

Signed-off-by: Gerd Hoffmann <kraxel@redhat.com>
---
 content.tex | 2 ++
 1 file changed, 2 insertions(+)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index be18234..d41c2f8 100644
--- a/content.tex
+++ b/content.tex
@@ -5325,6 +5325,8 @@ descriptor for the \field{sense_len}, \field{residual},
 \field{status_qualifier}, \field{status}, \field{response} and
 \field{sense} fields.
 
+\input{virtio-gpu.tex}
+
 \chapter{Reserved Feature Bits}\label{sec:Reserved Feature Bits}
 
 Currently these device-independent feature bits defined:
-- 
cgit v1.2.3

