From 0bc9dbd2b501b8e37410344fb9dc645537142ff2 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 25 Mar 2015 17:07:04 +0000
Subject: Change 4.1.5.1.2.1 to device requirement

4.1.5.1.2.1 is incorrectly labelled as a driver requirement; it's
self-evidently referring to the device.

VIRTIO-133

Signed-off-by: Rusty Russell <rusty@rustcorp.com.au>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@488 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 1b682d8..947e4b0 100644
--- a/content.tex
+++ b/content.tex
@@ -1631,7 +1631,7 @@ Structure PCI capabilities as detailed in \ref{sec:Virtio Transport Options / Vi
 
 \paragraph{Non-transitional Device With Legacy Driver}\label{sec:Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
 
-\drivernormative{\subparagraph}{Non-transitional Device With Legacy Driver}{Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
+\devicenormative{\subparagraph}{Non-transitional Device With Legacy Driver}{Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
 
 Non-transitional devices, on a platform where a legacy driver for
 a legacy device with the same ID might have previously existed,
-- 
cgit v1.2.3

