From 15d8b243843e164e1914b5a7b6d633fda2e87351 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 11 Oct 2015 14:55:13 +0000
Subject: virtqueues: fix trivial typo

Signed-off-by: Greg Kurz <gkurz@linux.vnet.ibm.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@540 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index d989d98..bc7455b 100644
--- a/content.tex
+++ b/content.tex
@@ -522,7 +522,7 @@ VRING_AVAIL_F_NO_INTERRUPT, but the layout and value were identical.
 If the VIRTIO_F_EVENT_IDX feature bit is not negotiated,
 the \field{flags} field in the available ring offers a crude mechanism for the driver to inform
 the device that it doesn't want interrupts when buffers are used.  Otherwise
-\field{used_event} is a more performant alterative where the driver
+\field{used_event} is a more performant alternative where the driver
 specifies how far the device can progress before interrupting.
 
 Neither of these interrupt suppression methods are reliable, as they
-- 
cgit v1.2.3

