From 173247e46945475ac9ddf2ed8d286d685a971d80 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 10 Feb 2014 10:32:46 +0000
Subject: patch feedback-8-5.patch

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@221 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 907ea5a..1a86bf9 100644
--- a/content.tex
+++ b/content.tex
@@ -1047,13 +1047,13 @@ struct virtio_pci_common_cfg {
         Note: this is *not* an offset in bytes. See \ref{sec:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Notification capability} below.
 
 \item[\field{queue_desc}]
-        The driver writes the physical address of Descriptor Table here.
+        The driver writes the physical address of Descriptor Table here.  See section \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
 
 \item[\field{queue_avail}]
-        The driver writes the physical address of Available Ring here.
+        The driver writes the physical address of Available Ring here.  See section \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
 
 \item[\field{queue_used}]
-        The driver writes the physical address of Used Ring here.
+        The driver writes the physical address of Used Ring here.  See section \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
 \end{description}
 
 \subsubsection{Notification structure layout}\label{sec:Virtio Transport Options / Virtio Over PCI Bus / PCI Device Layout / Notification capability}
-- 
cgit v1.2.3

