From 1c8e63c8eb4fdc388715800ffa8d86ca1d480f6e Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 2 Mar 2014 21:34:50 +0000
Subject: legacy: make message framing normative

Change accepted on VIRTIO TC Meeting, 3 December 2013

TODO: we really should be more specific

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@292 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 15005fc..7d6ce02 100644
--- a/content.tex
+++ b/content.tex
@@ -391,7 +391,7 @@ addition, the specification for virtio_blk SCSI commands required
 intuiting field lengths from frame boundaries (see
  \ref{sec:Device Types / Block Device / Device Operation / Legacy Interface: Device Operation}~\nameref{sec:Device Types / Block Device / Device Operation / Legacy Interface: Device Operation})
 
-It is thus recommended that when using legacy interfaces, transitional
+It is thus RECOMMENDED that when using legacy interfaces, transitional
 drivers be conservative in their assumptions, unless the
 VIRTIO_F_ANY_LAYOUT feature is accepted.
 
-- 
cgit v1.2.3

