From 1e1210c5b0d8afaea3369fd6bb1751162015ab2f Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 22 Dec 2014 11:36:27 +0000
Subject: ccw: two-stage indicators for legacy devices

Some legacy devices will support two-stage queue indicators and therefore
won't reject CCW_CMD_SET_IND_ADAPTER. Note this.

VIRTIO-127

Signed-off-by: Cornelia Huck <cornelia.huck@de.ibm.com>
Reviewed-by: Michael S. Tsirkin <mst@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@450 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 7 +++++--
 1 file changed, 5 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index d2d9ae7..952b605 100644
--- a/content.tex
+++ b/content.tex
@@ -2742,8 +2742,11 @@ command reject to any subsequent CCW_CMD_SET_IND_ADAPTER command.
 
 \paragraph{Legacy Interfaces: A Note on Setting Up Indicators}\label{sec:Virtio Transport Options / Virtio over channel I/O / Device Initialization / Setting Up Indicators / Legacy Interfaces: A Note on Setting Up Indicators}
 
-Legacy devices will only support classic queue indicators; they will
-reject CCW_CMD_SET_IND_ADAPTER as they don't know that command.
+In some cases, legacy devices will only support classic queue indicators;
+in that case, they will reject CCW_CMD_SET_IND_ADAPTER as they don't know that
+command. Some legacy devices will support two-stage queue indicators, though,
+and a driver will be able to successfully use CCW_CMD_SET_IND_ADAPTER to set
+them up.
 
 \subsection{Device Operation}\label{sec:Virtio Transport Options / Virtio over channel I/O / Device Operation}
 
-- 
cgit v1.2.3

