From 23b092a423decab7435a261e46855dad72c01aff Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 19 Feb 2014 01:22:38 +0000
Subject: net: fix incorrect reference.

It pointed into the block section for some reason.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@250 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 7e112c7..e7f581b 100644
--- a/content.tex
+++ b/content.tex
@@ -2743,7 +2743,7 @@ VIRTIO_NET_F_MRG_RXBUF case.
 
 Often a driver will suppress transmission interrupts using the
 VRING_AVAIL_F_NO_INTERRUPT flag
- (see \ref{sec:Device Types / Block Device}~\nameref{sec:Device Types / Block Device})
+ (see \ref{sec:General Initialization And Device Operation / Device Operation / Receiving Used Buffers From The Device}~\nameref{sec:General Initialization And Device Operation / Device Operation / Receiving Used Buffers From The Device})
 and check for used packets in the transmit path of following
 packets.
 
-- 
cgit v1.2.3

