From 24d4065de2b1c4c500b07cde6b535abe5713a5f9 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 12 May 2014 01:58:36 +0000
Subject: VIRTIO-96: Assign device id to virtio input

Assign device id to virtio input

As passed at meeting 2014-05-06:
	https://lists.oasis-open.org/archives/virtio/201405/msg00016.html

Signed-off-by: Gerd Hoffmann <kraxel@redhat.com>
Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@370 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 ++
 1 file changed, 2 insertions(+)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 17599f3..a745599 100644
--- a/content.tex
+++ b/content.tex
@@ -2838,6 +2838,8 @@ Device ID  &  Virtio Device    \\
 \hline
 17         &   Timer/Clock device \\
 \hline
+18         &   Input device \\
+\hline
 \end{tabular}
 
 Some of the devices above are unspecified by this document,
-- 
cgit v1.2.3

