From 31e5624a6fe50799ab61c9e5bacb0fc997331cf9 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 4 Aug 2014 12:45:34 +0000
Subject: legacy: consistently use past tense

Paragraph with general description of feature negotiation
for legacy devices mixed present and past tense.
As rest of legacy sections all use past tense,
fix the only instance of the present tense:
s/do/did/ for consistency.

It might be argued that legacy devices still have these
properties so present tense is more appropriate, on the
other hand, using the past tense helps stress the fact
that current spec does not attempt to fully describe the legacy
device/driver behaviour: this text is only here to serve as
motivation for the transitional device/driver requirements.

VIRTIO-112

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@413 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 0f7326e..cb2a89d 100644
--- a/content.tex
+++ b/content.tex
@@ -707,7 +707,7 @@ driver MUST NOT continue initialization in that case.
 The driver MUST NOT notify the device before setting DRIVER_OK.
 
 \subsection{Legacy Interface: Device Initialization}\label{sec:General Initialization And Device Operation / Device Initialization / Legacy Interface: Device Initialization}
-Legacy devices do not support the FEATURES_OK status bit, and thus did
+Legacy devices did not support the FEATURES_OK status bit, and thus did
 not have a graceful way for the device to indicate unsupported feature
 combinations.  It also did not provide a clear mechanism to end
 feature negotiation, which meant that devices finalized features on
-- 
cgit v1.2.3

