From 3745a61c4fd3e13099d1fd0668063d347d4cc0db Mon Sep 17 00:00:00 2001
From: hornet <hornet@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 26 Feb 2014 16:04:48 +0000
Subject: mmio: Fix Device Tree example

Minor fix: the size of 0x100 was obviously wrong,
as it didn't allow for configuration space.

Signed-off-by: Pawel Moll <pawel.moll@arm.com>


git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@283 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index c4cbe81..240bafa 100644
--- a/content.tex
+++ b/content.tex
@@ -1681,10 +1681,10 @@ and interrupt(s) used.  The suggested binding for systems using
 flattened device trees is shown in this example:
 
 \begin{lstlisting}
-// EXAMPLE: virtio_block device taking 256 bytes at 0x1e000, interrupt 42.
+// EXAMPLE: virtio_block device taking 512 bytes at 0x1e000, interrupt 42.
 virtio_block@1e000 {
         compatible = "virtio,mmio";
-        reg = <0x1e000 0x100>;
+        reg = <0x1e000 0x200>;
         interrupts = <42>;
 }
 \end{lstlisting}
-- 
cgit v1.2.3

