From 46b77c20ceca7df92f4d889348dbe13d0904539a Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Thu, 27 Feb 2014 00:28:15 +0000
Subject: Fixed path of linux version of virtio_ring.h

Signed-off-by: Holm Rauchfuss <holm.rauchfuss@huawei.com>
Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@286 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index d03a33f..ef81a4e 100644
--- a/content.tex
+++ b/content.tex
@@ -586,7 +586,7 @@ The device MUST handle spurious notifications from the driver.
 
 The Linux Kernel Source code contains the definitions above and
 helper routines in a more usable form, in
-include/linux/virtio_ring.h. This was explicitly licensed by IBM
+include/uapi/linux/virtio_ring.h. This was explicitly licensed by IBM
 and Red Hat under the (3-clause) BSD license so that it can be
 freely used by all other projects, and is reproduced (with slight
 variation to remove Linux assumptions) in \ref{sec:virtio-ring.h}~\nameref{sec:virtio-ring.h}.
-- 
cgit v1.2.3

