From 4b7a5dcdecb5947a68e9819588f66772b8d46a35 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 2 Mar 2014 21:35:12 +0000
Subject: legacy pci layout: extra confirmance statement

Change accepted on VIRTIO TC Meeting, 3 December 2013

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@294 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index a9dc037..b1a293f 100644
--- a/content.tex
+++ b/content.tex
@@ -1447,8 +1447,10 @@ enabled, device specific configuration starts at byte offset 20 in virtio
 header.  ie. once you enable MSI-X on the device, the other fields move.
 If you turn it off again, they move back!
 
-Immediately following these general headers, there may be
-device-specific headers:
+When using the legacy interface, both transitional
+devices and drivers MUST assume that
+the device-specific configuration space
+immediately follows these general headers:
 
 \begin{tabular}{|l||l|l|}
 \hline
-- 
cgit v1.2.3

