From 5223bff5c7f8b7cbbe2908202ef618dd09633636 Mon Sep 17 00:00:00 2001
From: hornet <hornet@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 26 Feb 2014 16:12:00 +0000
Subject: mmio: Clarify normative requirement on QueueNum

Minor fix: add explicit reference to QueueNumMax in the
normative paragraph describing QueueNum.

Signed-off-by: Pawel Moll <pawel.moll@arm.com>


git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@285 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 1e2480b..d03a33f 100644
--- a/content.tex
+++ b/content.tex
@@ -1904,7 +1904,7 @@ Before reading from \field{DeviceFeatures}, the driver MUST write a value to \fi
 Before writing to the \field{DriverFeatures} register, the driver MUST write a value to the \field{DriverFeaturesSel} register.
 
 The driver MUST write a value to \field{QueueNum} which is less than
-or equal to the value presented by the device.
+or equal to the value presented by the device in \field{QueueNumMax}.
 
 When \field{QueueReady} is not zero, the driver MUST NOT access
 \field{QueueNum}, \field{QueueDescLow}, \field{QueueDescHigh},
-- 
cgit v1.2.3

