From 525835c50ef60324c9cb14bf3b8a8bc7839f77d6 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 25 Mar 2015 17:06:40 +0000
Subject: ISR status: Fix incorrect diagram

ISR status capability diagram has the "Device Configuration
Interrupt " as bit 0, and the "Queue Interrupt" as bit 1. This is
the wrong way around: it disagrees with the legacy
implementations, as well as the spec elsewhere.

All current guests correctly follow the text, fix
up the diagram to match.

VIRTIO-130

Signed-off-by: Rusty Russell <rusty@rustcorp.com.au>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@487 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index c9440a4..1b682d8 100644
--- a/content.tex
+++ b/content.tex
@@ -1415,7 +1415,7 @@ change interrupts and normal virtqueue interrupts:
 \hline
 Bits       & 0                               & 1               &  2 to 31 \\
 \hline
-Purpose    & Device Configuration Interrupt  & Queue Interrupt & Reserved \\
+Purpose    & Queue Interrupt  & Device Configuration Interrupt & Reserved \\
 \hline
 \end{tabular}
 
-- 
cgit v1.2.3

