From 568383447cd3bd83d5ecfbd116ab6c0f769094cb Mon Sep 17 00:00:00 2001
From: hornet <hornet@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Fri, 3 Jan 2014 17:57:34 +0000
Subject: mmio: Obviously wrong notification register name

The "4.2.3.3 Notifying The Device" section said "writing
the index of the updated queue to the QueueNum". This
is obviously wrong - should read "QueueNotify".

Signed-off-by: Pawel Moll <pawel.moll@arm.com>



git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@179 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 797ee3e..7091bf4 100644
--- a/content.tex
+++ b/content.tex
@@ -1645,7 +1645,7 @@ The driver MUST initialize the virtual queue in the following way:
 \subsubsection{Notifying The Device}\label{sec:Virtio Transport Options / Virtio Over MMIO / MMIO-specific Initialization And Device Operation / Notifying The Device}
 
 The driver MUST notify the device about new buffers being available in
-a queue by writing the index of the updated queue to the QueueNum register.
+a queue by writing the index of the updated queue to the QueueNotify register.
 
 \subsubsection{Notifications From The Device}\label{sec:Virtio Transport Options / Virtio Over MMIO / MMIO-specific Initialization And Device Operation / Notifications From The Device}
 
-- 
cgit v1.2.3

