From 61e96946bb276abd485cf4f605f9f8a6efc3e005 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 2 Mar 2014 21:34:16 +0000
Subject: legacy: clarify general note on endian-ness

Change accepted on VIRTIO TC Meeting, 3 December 2013

this is a non normative section.
we merely mention that details are given
for each device.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@289 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 1 +
 1 file changed, 1 insertion(+)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 7eb08d0..744ba34 100644
--- a/content.tex
+++ b/content.tex
@@ -230,6 +230,7 @@ by the device.
 
 Note that for legacy interfaces, device configuration space is generally the
 guest's native endian, rather than PCI's little-endian.
+The correct endian-ness is documented explicitly for each device.
 
 \subsection{Legacy Interface: Device Configuration Space}\label{sec:Basic Facilities of a Virtio Device / Device Configuration Space / Legacy Interface: Device Configuration Space}
 
-- 
cgit v1.2.3

