From 64d4d1a8d09fff84b5de6cc30eda359ba5275faf Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 2 Mar 2014 21:37:38 +0000
Subject: initialization: minor clarification

Change accepted on VIRTIO TC Meeting, 3 December 2013

"it" could refer to failed bit or the driver.
clarify.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@307 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index c98648b..b0876b5 100644
--- a/content.tex
+++ b/content.tex
@@ -52,7 +52,7 @@ initialization sequence specified in
 Initialization}.
 The driver MUST NOT clear a
 \field{device status} bit.  If the driver sets the FAILED bit,
-it MUST reset the device before attempting to re-initialize.
+the driver MUST later reset the device before attempting to re-initialize.
 
 \devicenormative{\subsection}{Device Status Field}{Basic Facilities of a Virtio Device / Device Status Field}
 The device MUST initialize \field{device status} to 0 upon reset.
-- 
cgit v1.2.3

