From 65853394e08c2f97ae68594496d0f187aeb65590 Mon Sep 17 00:00:00 2001
From: pbonzini <pbonzini@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 16 Jun 2014 11:54:22 +0000
Subject: fix erroneous reference to Subsystem Device ID

Subsystem device ID only exists for PCI.

Signed-off-by: Paolo Bonzini <pbonzini@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@383 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 9670976..56f58fa 100644
--- a/content.tex
+++ b/content.tex
@@ -101,7 +101,7 @@ Feature bits are allocated as follows:
 \end{description}
 
 \begin{note}
-For example, feature bit 0 for a network device (i.e. Subsystem
+For example, feature bit 0 for a network device (i.e.
 Device ID 1) indicates that the device supports checksumming of
 packets.
 \end{note}
-- 
cgit v1.2.3

