From 65c4282c789c43ec7a6fb600afb5f1df0aa67146 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 19 Feb 2014 01:23:01 +0000
Subject: Gratuitous Packet Sending: clarify wording.

The device can ask, not the driver.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@251 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index e7f581b..2928eb8 100644
--- a/content.tex
+++ b/content.tex
@@ -2936,7 +2936,7 @@ native endian of the guest rather than (necessarily) little-endian.
 \paragraph{Gratuitous Packet Sending}\label{sec:Device Types / Network Device / Device Operation / Control Virtqueue / Gratuitous Packet Sending}
 
 If the driver negotiates the VIRTIO_NET_F_GUEST_ANNOUNCE (depends
-on VIRTIO_NET_F_CTRL_VQ), it can ask the driver to send gratuitous
+on VIRTIO_NET_F_CTRL_VQ), the device can ask the driver to send gratuitous
 packets; this is usually done after the guest has been physically
 migrated, and needs to announce its presence on the new network
 links. (As hypervisor does not have the knowledge of guest
-- 
cgit v1.2.3

