From 6620a37c5879805026781e1fe1981faa57700116 Mon Sep 17 00:00:00 2001
From: hornet <hornet@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 16 Dec 2013 11:31:42 +0000
Subject: 2.3.2 MMIO: Configuration space offset corrected

The offset in the MMIO configuration space description
(table 4.1) became wrong at some time (0x0fff). Fixed.

Signed-off-by: Pawel Moll <pawel.moll@arm.com>



git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@177 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 0089846..797ee3e 100644
--- a/content.tex
+++ b/content.tex
@@ -1590,9 +1590,9 @@ All register values are organized as Little Endian.
   }
   \hline 
   \mmioreg{Config}{Configuration space}{0x100+}{RW}{
-    Device-specific configuration space starts at an offset 0x0ff
+    Device-specific configuration space starts at the offset 0x100
     and is accessed with byte alignment. Its meaning and size
-    depends on the device and the driver.
+    depend on the device and the driver.
   }
   \hline
 \end{longtable}
-- 
cgit v1.2.3

