From 77cb18f8f2763e28d9a40abcc677c36b9d213050 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 5 Mar 2014 11:11:44 +0000
Subject: transitional driver features: fix typos noted by Rusty

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@311 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index a509b20..439a972 100644
--- a/content.tex
+++ b/content.tex
@@ -4862,7 +4862,7 @@ Transitional devices MAY offer the following:
 \end{description}
 
 Transitional devices MUST offer, and if offered by the device
-traditional drivers MUST negotiate the following:
+transitional drivers MUST accept the following:
 \begin{description}
 \item[VIRTIO_F_ANY_LAYOUT (27)] This feature indicates that the device
   accepts arbitrary descriptor layouts, as described in Section
-- 
cgit v1.2.3

