From 827569aae7633df9053758304c3e5f2b0f5a53ab Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Tue, 3 Dec 2013 06:46:53 +0000
Subject: Remove suggestion to use old virtualization list for number
 assignment.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@154 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 6 ++----
 1 file changed, 2 insertions(+), 4 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 29ae708..8cfc36f 100644
--- a/content.tex
+++ b/content.tex
@@ -4018,10 +4018,8 @@ are atomically writable.
 
 \section{What Device Number?}\label{sec:Creating New Device Types / What Device Number?}
 
-Currently device numbers are assigned quite freely: a simple
-request mail to the author of this document or the Linux
-virtualization mailing list\footnote{https://lists.linux-foundation.org/mailman/listinfo/virtualization
-} will be sufficient to secure a unique one.
+Device numbers can be reserved by the OASIS committee: email
+virtio-dev@lists.oasis-open.org to secure a unique one.
 
 Meanwhile for experimental drivers, use 65535 and work backwards.
 
-- 
cgit v1.2.3

