From 99aacdaa9d8c60950bde56ddddafede496d7e7c7 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 29 Apr 2015 11:09:39 +0000
Subject: entropy device: typo fix

The driver MUST examine the length written by the driver

makes no sense. length is written by the device.

VIRTIO-142

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@523 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 7e46b7d..11015a5 100644
--- a/content.tex
+++ b/content.tex
@@ -4349,7 +4349,7 @@ by random data by the device.
 
 The driver MUST NOT place driver-readable buffers into the queue.
 
-The driver MUST examine the length written by the driver to determine
+The driver MUST examine the length written by the device to determine
 how many random bytes were received.
 
 \devicenormative{\subsubsection}{Device Operation}{Device Types / Entropy Device / Device Operation}
-- 
cgit v1.2.3

