From a75a70b428f33cf2b684f09a4b0dcc7985726b02 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 22 Apr 2015 08:25:52 +0000
Subject: mark diff for non-transitional with legacy

latexdiff doesn't handle changing labels well,
causes latex unresolved reference errors.

opencode and mark up diff manually.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@507 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 14 +++++++++++++-
 1 file changed, 13 insertions(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 5a1a989..48d735d 100644
--- a/content.tex
+++ b/content.tex
@@ -1649,7 +1649,19 @@ Such buggy drivers are not currently known to be used in
 production.
 \end{note}
 
-\devicenormative{\paragraph}{Non-transitional Device With Legacy Driver}{Virtio Transport Options / Virtio Over PCI Bus / PCI-specific Initialization And Device Operation / Device Initialization / Non-transitional Device With Legacy Driver}
+\subparagraph{
+\DIFdeltextcstwo{Driver Requirements: Non-transitional Device With Legacy Driver}
+\DIFaddtextcstwo{Device Requirements: Non-transitional Device With Legacy Driver}
+}
+\label{drivernormative:Virtio Transport Options / Virtio Over PCI
+Bus / PCI-specific Initialization And Device Operation /
+Device Initialization / Non-transitional Device With Legacy
+Driver}
+\label{devicenormative:Virtio Transport Options / Virtio Over PCI
+Bus / PCI-specific Initialization And Device Operation /
+Device Initialization / Non-transitional Device With Legacy
+Driver}
+
 Non-transitional devices, on a platform where a legacy driver for
 a legacy device with the same ID (including PCI Revision, Device
 and Vendor IDs) is known to have previously existed,
-- 
cgit v1.2.3

