From b03fa34f2ff51894d09050b2fc5cc23973f191d5 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 2 Dec 2013 12:30:46 +0000
Subject: pci: fix config notify bit.

The Linux code uses 0x2, so I assume second lowest bit is right...

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@146 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index a911383..a94d0d0 100644
--- a/content.tex
+++ b/content.tex
@@ -1290,7 +1290,7 @@ state, as reflected in the virtio header in the PCI configuration
 space. In this case:
 
 1. If MSI-X capability is disabled: an interrupt is delivered and
-  the second highest bit is set in the ISR Status field to
+  the second lowest bit is set in the ISR Status field to
   indicate that the driver should re-examine the configuration
   space.  Note that a single interrupt can indicate both that one
   or more virtqueue has been used and that the configuration
-- 
cgit v1.2.3

