From b789c0ab2ffca627f908765bb34408b5f3f89d85 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 26 Feb 2014 03:20:46 +0000
Subject: Feedback: add normative marker.

From http://docs.oasis-open.org/templates/TCHandbook/ConformanceGuidelines.html:
   Normative statements MUST be referenceable so that a statement may be
   referenced from another part of a specification, but more importantly
   so they can be referenced from Conformance Clauses.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@265 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 ++
 1 file changed, 2 insertions(+)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 6ab0caa..1589ddb 100644
--- a/content.tex
+++ b/content.tex
@@ -40,11 +40,13 @@ following bits are defined:
   even a fatal error during device operation.
 \end{description}
 
+\drivernormative{Basic Facilities of a Virtio Device / Device Status Field}
 The driver MUST update \field{device status} in the order above to
 indicate the driver's progress.  The driver MUST NOT clear a
 \field{device status} bit.  If the driver sets the FAILED bit,
 it MUST reset the device before attempting to re-initialize.
 
+\devicenormative{Basic Facilities of a Virtio Device / Device Status Field}
 The device MUST initialize \field{device status} to 0 upon reset.
 
 \section{Feature Bits}\label{sec:Basic Facilities of a Virtio Device / Feature Bits}
-- 
cgit v1.2.3

