From cf4c71d5652997d4f3032955fbcc2d52f2970df9 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 26 Feb 2014 03:17:29 +0000
Subject: Feedback: TAB-555 Bad sub-sectioning (VIRTIO-80)

Reported-by: Patrick Durusau <patrick@durusau.net>
Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@257 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 1250a90..8cd408b 100644
--- a/content.tex
+++ b/content.tex
@@ -4332,10 +4332,6 @@ Currently there are four device-independent feature bits defined:
   drivers.
 \end{description}
 
-In addition, bit 30 is used by qemu's implementation to check for experimental
-early versions of virtio which did not perform correct feature negotiation,
-and should not be used.
-
 \section{Legacy Interface: Reserved Feature Bits}\label{sec:Reserved Feature Bits / Legacy Interface: Reserved Feature Bits}
 
 Legacy or transitional devices may offer the following:
@@ -4355,6 +4351,10 @@ Legacy or transitional devices may offer the following:
 \item[VIRTIO_F_ANY_LAYOUT (27)] This feature indicates that the device
   accepts arbitrary descriptor layouts, as described in Section
   \ref{sec:Basic Facilities of a Virtio Device / Virtqueues / Message Framing / Legacy Interface: Message Framing}~\nameref{sec:Basic Facilities of a Virtio Device / Virtqueues / Message Framing / Legacy Interface: Message Framing}.
+
+\item[UNUSED (30)] Bit 30 is used by qemu's implementation to check
+  for experimental early versions of virtio which did not perform
+  correct feature negotiation, and should not be used.
 \end{description}
 
 \chapter{virtio_ring.h}\label{sec:virtio-ring.h}
-- 
cgit v1.2.3

