From da40d31b92d562cc5a98585aa2547511d1c75078 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 25 Nov 2013 12:27:38 +0000
Subject: content.tex: fix up cross-reference to S390

make it a hyper-link.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@119 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index e450d88..7766fb8 100644
--- a/content.tex
+++ b/content.tex
@@ -1785,7 +1785,7 @@ virtio:
 \end{lstlisting}
 
 The virtio-ccw device acts like a normal channel device, as specified
-in [S390 PoP] and [S390 Common I/O]. In particular:
+in \hyperref[intro:S390 PoP]{[S390 PoP]} and \hyperref[intro:S390 Common I/O]{[S390 Common I/O]}. In particular:
 
 - A device must post a unit check with command reject for any command
   it does not support.
-- 
cgit v1.2.3

