From e81e656586eb6c13a68a846cf67026bd4d970e47 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sat, 31 May 2014 21:16:15 +0000
Subject: NEEDS_RESET: trivial clarification

If device sets NEEDS_RESET before DRIVER_OK, it
can't send notifications to driver.
Make this clear.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@374 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 6d6a756..b82748a 100644
--- a/content.tex
+++ b/content.tex
@@ -74,7 +74,7 @@ The device MUST initialize \field{device status} to 0 upon reset.
 The device MUST NOT consume buffers or notify the driver before DRIVER_OK.
 
 \label{sec:Basic Facilities of a Virtio Device / Device Status Field / DEVICENEEDSRESET}The device SHOULD set DEVICE_NEEDS_RESET when it enters an error state
-that a reset is needed.  After it sets DEVICE_NEEDS_RESET, the device
+that a reset is needed.  If DRIVER_OK is set, after it sets DEVICE_NEEDS_RESET, the device
 MUST send a device configuration change notification to the driver.
 
 \section{Feature Bits}\label{sec:Basic Facilities of a Virtio Device / Feature Bits}
-- 
cgit v1.2.3

