From f15b53cd97a939b97f215b43e0d8a6d02603262c Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 11 Oct 2015 14:56:13 +0000
Subject: virtio-blk: flush: Fix driver vs. device typo

This is a simple non-material change.

Signed-off-by: Paolo Bonzini <pbonzini@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@542 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index bc35813..4be0f7d 100644
--- a/content.tex
+++ b/content.tex
@@ -4189,7 +4189,7 @@ A device MUST set the \field{status} byte to VIRTIO_BLK_S_IOERR
 for a write request if the VIRTIO_BLK_F_RO feature if offered, and MUST NOT
 write any data.
 
-Upon receipt of a VIRTIO_BLK_T_FLUSH request, the driver SHOULD ensure
+Upon receipt of a VIRTIO_BLK_T_FLUSH request, the device SHOULD ensure
 that any writes which were completed are committed to non-volatile storage.
 
 \subsubsection{Legacy Interface: Device Operation}\label{sec:Device Types / Block Device / Device Operation / Legacy Interface: Device Operation}
-- 
cgit v1.2.3

