From f1b4fcc103575c6fea9eeb62ba86a59d3ba4ca6f Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Tue, 23 Dec 2014 19:24:34 +0000
Subject: add legacy tag for makediff between cs02 and cs01

This is here merely as a work-around for latex-diff producing
broken cross-references when labels are re-named.
Not needed on trunk.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@454 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 2 ++
 1 file changed, 2 insertions(+)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 56c9807..f9300e6 100644
--- a/content.tex
+++ b/content.tex
@@ -3034,6 +3034,7 @@ upon further investigation it became clear that multiple bits
 were needed.
 
 \subsection{Device configuration layout}\label{sec:Device Types / Network Device / Device configuration layout}
+\label{sec:Device Types / Block Device / Feature bits / Device configuration layout}
 
 Three driver-read-only configuration fields are currently defined. The \field{mac} address field
 always exists (though is only valid if VIRTIO_NET_F_MAC is set), and
@@ -3078,6 +3079,7 @@ assume the link is active, otherwise it SHOULD read the link status from
 the bottom bit of \field{status}.
 
 \subsubsection{Legacy Interface: Device configuration layout}\label{sec:Device Types / Network Device / Device configuration layout / Legacy Interface: Device configuration layout}
+\label{sec:Device Types / Block Device / Feature bits / Device configuration layout / Legacy Interface: Device configuration layout}
 When using the legacy interface, transitional devices and drivers
 MUST format \field{status} and
 \field{max_virtqueue_pairs} in struct virtio_net_config
-- 
cgit v1.2.3

