From f324e9e4fc89c9586b3f7d7c616c23b104b197e0 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Thu, 23 Jan 2014 02:10:40 +0000
Subject: Formatting: fix feature bits for console device.

Make them a description list like every other device.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@191 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index b038b0c..17d1bd7 100644
--- a/content.tex
+++ b/content.tex
@@ -3218,12 +3218,14 @@ data and outgoing characters are placed in the transmit queue.
 
 \subsection{Feature bits}\label{sec:Device Types / Console Device / Feature bits}
 
-  VIRTIO_CONSOLE_F_SIZE (0) Configuration cols and rows fields
+\begin{description}
+\item[VIRTIO_CONSOLE_F_SIZE (0)] Configuration cols and rows fields
     are valid.
 
-  VIRTIO_CONSOLE_F_MULTIPORT(1) Device has support for multiple
+\item[VIRTIO_CONSOLE_F_MULTIPORT (1)] Device has support for multiple
     ports; configuration fields nr_ports and max_nr_ports are
     valid and control virtqueues will be used.
+\end{description}
 
 \subsection{Device configuration layout}\label{sec:Device Types / Console Device / Device configuration layout}
 
-- 
cgit v1.2.3

