From f37b614cd3760036d9302f1e9bf985ec19892586 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Mon, 2 Dec 2013 12:30:30 +0000
Subject: Terminology: Device and driver, not host and guest.

We've mixed both together, whereas from a spec-reader point of view,
"driver" and "device" is probably clearer.

CCW part incorporated:

  Switch the parts of the virtio-ccw specification that did not already
  to device/driver instead of guest/host. For more general discussions,
  host/guest is kept (like when talking about guest<->host notifications
  in general). This should make things more consistent.

  Signed-off-by: Cornelia Huck <cornelia.huck@de.ibm.com>

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@145 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 introduction.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'introduction.tex')

diff --git a/introduction.tex b/introduction.tex
index 241caee..60846b9 100644
--- a/introduction.tex
+++ b/introduction.tex
@@ -14,7 +14,7 @@ inter-guest communication) requires copying.
 
   Efficient: Virtio devices consist of rings of descriptors
   for input and output, which are neatly separated to avoid cache
-  effects from both guest and device writing to the same cache
+  effects from both driver and device writing to the same cache
   lines.
 
   Standard: Virtio makes no assumptions about the environment in which
-- 
cgit v1.2.3

