From 716fe0421d20d12f71c1fec589dffa86e4219a03 Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Thu, 13 Mar 2014 03:11:55 +0000
Subject: VIRTIO-81: MUST vs must

Clean up the remaining lowercase "musts".  We actually introduce a
new normative section in the balloon; for the rest we clarify them
one way or another.

Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@318 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 newdevice.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'newdevice.tex')

diff --git a/newdevice.tex b/newdevice.tex
index 5e07b79..c7e6221 100644
--- a/newdevice.tex
+++ b/newdevice.tex
@@ -22,8 +22,8 @@ configuration information (the network device does this for filtering,
 otherwise the table in the config space could potentially be very
 large).
 
-Devices must not assume that configuration fields over 32 bits wide
-are atomically writable by the driver.
+Remember that configuration fields over 32 bits wide might not be
+atomically writable by the driver.
 
 \section{What Device Number?}\label{sec:Creating New Device Types / What Device Number?}
 
-- 
cgit v1.2.3

