From 545c92fe0fef159047d9a0d3ca3807613fe8e3c2 Mon Sep 17 00:00:00 2001
From: Christoffer Dall <christoffer.dall@arm.com>
Date: Tue, 22 May 2018 21:11:05 +0200
Subject: split-ring: Fix typo in used ring description

Only the device updates the used ring.

This looks like a typo as a result of copy-paste from the description of
the Available Ring.

Fixes: https://github.com/oasis-tcs/virtio-spec/issues/12
Signed-off-by: Christoffer Dall <christoffer.dall@arm.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Reviewed-by: Laszlo Ersek <lersek@redhat.com>
Reviewed-by: Stefan Hajnoczi <stefanha@redhat.com>
---
 split-ring.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'split-ring.tex')

diff --git a/split-ring.tex b/split-ring.tex
index df278fe..2267863 100644
--- a/split-ring.tex
+++ b/split-ring.tex
@@ -417,7 +417,7 @@ overwritten the bytes which were in that buffer, this could leak the
 contents of freed memory from other processes to the application.
 \end{note}
 
-\field{idx} field indicates where the driver would put the next descriptor
+\field{idx} field indicates where the device would put the next descriptor
 entry in the ring (modulo the queue size). This starts at 0, and increases.
 
 \begin{note}
-- 
cgit v1.2.3

