From ae98c6bc21bccee8ef9b9415f68f965797d5a082 Mon Sep 17 00:00:00 2001
From: "Michael S. Tsirkin" <mst@redhat.com>
Date: Fri, 9 Mar 2018 23:23:32 +0200
Subject: content: generalize transport ring part naming

Replace descriptor table/available ring/used ring
with descriptor area/driver area/device area
in all transports.

Document what's in which area.

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Reviewed-by: Cornelia Huck <cohuck@redhat.com>
Approved-by: https://www.oasis-open.org/apps/org/workgroup/virtio/ballot.php?id=3177
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/3
---
 split-ring.tex | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

(limited to 'split-ring.tex')

diff --git a/split-ring.tex b/split-ring.tex
index 404660b..9601a53 100644
--- a/split-ring.tex
+++ b/split-ring.tex
@@ -15,9 +15,9 @@ of the queue.
 Each virtqueue consists of three parts:
 
 \begin{itemize}
-\item Descriptor Table
-\item Available Ring
-\item Used Ring
+\item Descriptor Table - occupies the Descriptor Area
+\item Available Ring - occupies the Driver Area
+\item Used Ring - occupies the Device Area
 \end{itemize}
 
 where each part is physically-contiguous in guest memory,
-- 
cgit v1.2.3

