448 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-120: virtio:
fix used element size

General ring description lists size for
used ring elements as 4, it must be 8.

See \ref{sec:Basic Facilities of a Virtio Device / Virtqueues}.
 } \\
\hline
449 & 22 Doc 2014 & Cornelia Huck & {VIRTIO-125: block: fixup section levels
    The specification for the configuration layout for block devices
    should be its own subsection as for all other devices and not be
    hidden beneath "Feature bits".
    
    The normative sections for device operation should appear under
    the device operation section.
See \ref{sec:Device Types / Block Device / Device configuration
layout}.
 } \\
\hline
450 & 22 Dec 2014 & Cornelia Huck & {VIRTIO-127: ccw: two-stage
indicators for legacy devices

    Some legacy devices will support two-stage queue indicators
and therefore
    won't reject CCW_CMD_SET_IND_ADAPTER. Note this.

See \ref{sec:Virtio Transport Options / Virtio over channel I/O /
Device Initialization / Setting Up Indicators / Legacy
Interfaces: A Note on Setting Up Indicators}.
 } \\
\hline
452 & 22 Dec 2014 & Michael S. Tsirkin & {VIRTIO-115:
formatting: formatting: escape {\textbackslash}ldots in lstlisting

    {\textbackslash}ldots does not work within lstlisting, the result is
    {\textbackslash}ldots verbatim in the PDF output.

    To fix, make \$ an escape character, and escape the sequence:
    \${\textbackslash}ldots\$

See \ref{sec:Device Types / SCSI Host Device / Device Operation /
Device Operation: controlq}.
} \\
\hline
