From 1b94350c49c8f0425b32c2581e29787406e53034 Mon Sep 17 00:00:00 2001
From: mstsirkin <mstsirkin@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Sun, 15 Mar 2015 10:10:50 +0000
Subject: ccw: clarify basic channel commands

"Basic channel commands" seems to be not as clear as it could,
so let's spell out which channel commands we refer to.

VIRTIO-118

Signed-off-by: Cornelia Huck <cornelia.huck@de.ibm.com>

Approved unanimously:
https://www.oasis-open.org/apps/org/workgroup/virtio/ballot.php?id=2763
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio/branches/v1.0@480 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 10 ++++++++--
 1 file changed, 8 insertions(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index 1efe93a..ba5c63b 100644
--- a/content.tex
+++ b/content.tex
@@ -2381,8 +2381,14 @@ model corresponding to the attached virtio device's subsystem
 device ID, accessed via a virtual I/O subchannel and a virtual
 channel path of type 0x32. This proxy device is discoverable via
 normal channel subsystem device discovery (usually a STORE
-SUBCHANNEL loop) and answers to the basic channel commands, most
-importantly SENSE ID.
+SUBCHANNEL loop) and answers to the basic channel commands:
+
+\begin{itemize}
+\item NO-OPERATION (0x03)
+\item BASIC SENSE (0x04)
+\item TRANSFER IN CHANNEL (0x08)
+\item SENSE ID (0xe4)
+\end{itemize}
 
 For a virtio-ccw proxy device, SENSE ID will return the following
 information:
-- 
cgit v1.2.3

