From e3b04128ea5b9bcbedc2b1cc6f16615a8afe645a Mon Sep 17 00:00:00 2001
From: rusty <rusty@0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652>
Date: Wed, 12 Feb 2014 03:14:23 +0000
Subject: PCI: rearrange it all

This is the re-arrangement originally suggested by Rusty,
except I made some fixes and also tweaked a couple of places
where behaviour changes where suggested - if we want these,
they should go in separately.

Rearrange discovery section to make it clearer what goes on.
Wording changes MUST/MAY/etc.  Clarify cfg gateway use.  No
behavioural changes.

[ Merged "fixup! PCI: rearrange it all" --RR ]

As per minutes:
        https://lists.oasis-open.org/archives/virtio/201402/msg00121.html

Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Signed-off-by: Rusty Russell <rusty@au1.ibm.com>

git-svn-id: https://tools.oasis-open.org/version-control/svn/virtio@233 0c8fb4dd-22a2-4bb5-bc14-6c75a5f43652
---
 content.tex | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

(limited to 'content.tex')

diff --git a/content.tex b/content.tex
index abab16c..9c5b38f 100644
--- a/content.tex
+++ b/content.tex
@@ -1090,8 +1090,7 @@ the same Queue Notify address for all queues.
 The value cap.length presented by the device MUST be at least 2
 and MUST be large enough to support queue notification offsets
 for all supported queues in all possible configurations.
-For all queues, the value cap.length presented by the device MUST satisty:
-
+For all queues, the value cap.length presented by the device MUST satisfy:
 \begin{lstlisting}
 	cap.length >= queue_notify_off * notify_off_multiplier + 2
 \end{lstlisting}
-- 
cgit v1.2.3

