From 624fab7e85f9eb6f202ba8bd5d9bb38f9f089f99 Mon Sep 17 00:00:00 2001
From: Stefan Hajnoczi <stefanha@redhat.com>
Date: Wed, 14 Mar 2018 15:46:17 +0000
Subject: packed-ring: fix "the descriptor flags +field+ is updated"

Either it needs to be "the descriptors flags are update" (since "flags"
is plural) or "the descriptor flags field is updated".  Since "flags" is
a name of a specific field, I chose the latter solution.

Signed-off-by: Stefan Hajnoczi <stefanha@redhat.com>
Signed-off-by: Michael S. Tsirkin <mst@redhat.com>
Fixes: https://github.com/oasis-tcs/virtio-spec/issues/7
Approved-by: https://www.oasis-open.org/committees/ballot.php?id=3184
---
 packed-ring.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'packed-ring.tex')

diff --git a/packed-ring.tex b/packed-ring.tex
index 00befae..60b5559 100644
--- a/packed-ring.tex
+++ b/packed-ring.tex
@@ -567,8 +567,8 @@ the descriptor flags for the first descriptor
 (and the previous memory barrier) until after the rest of
 the descriptors have been initialized.
 
-Once the descriptor \field{flags} is updated by the driver, this exposes the
-descriptor and its contents.  The device MAY
+Once the descriptor \field{flags} field is updated by the driver, this exposes
+the descriptor and its contents.  The device MAY
 access the descriptor and any following descriptors the driver created and the
 memory they refer to immediately.
 
-- 
cgit v1.2.3

